
Oxford Semiconductor Ltd.
Reference driver for PCI ports

To use the Windows NT4 driver for a 2-serial port solution, perform
the following steps:-

1) Use the EEPROM to program the deviceID for function 0 to 0x950A
2) Replace the oxser.inf file in the WinNT4 directory with the version
   located in \doc\misc
3) Start up the system
4) Run the Install_Serial program from the WinNT4 directory
